With the help of an assistant, move the frame (A) against left or right, then lower the opposite side of the frame down. Keep the rear grab handle bracket (B) away from the frame while lowering it. Take care not to hang the frame on the bracket. With the help of an assistant, carefully remove the frame through the front door opening. Take care not to scratch the interior trim and body, or tear the seat covers. |